{
  "schema_version": 5,
  "saved_at": "2026-08-11T21:49:41.206027",
  "app_title": "TimbyrNode 2026.2.01",
  "app_version": "2026.2.01",
  "api_version": "25.1.5.1431",
  "cached_timber_bolts": {
    "1": {
      "name": "B1",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1731.7343355827634,
      "boltShearForces": [
        1731.7343355827634,
        1731.7343355827634
      ],
      "boltTensionForce": 0.0,
      "angle": 0.5892662167289983,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -1439.6750951604135,
          962.4133360522023,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "2": {
      "name": "B2",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 964.4406043977666,
      "boltShearForces": [
        964.4406043977666,
        964.4406043977666
      ],
      "boltTensionForce": 0.0,
      "angle": 1.5059464764859634,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          62.49999999999988,
          962.4133360522023,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "3": {
      "name": "B3",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1836.9669520234645,
      "boltShearForces": [
        1836.9669520234645,
        1836.9669520234645
      ],
      "boltTensionForce": 0.0,
      "angle": 0.5514400262273171,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          1564.675095160413,
          962.4133360522023,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "4": {
      "name": "B4",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1570.734030716259,
      "boltShearForces": [
        1570.734030716259,
        1570.734030716259
      ],
      "boltTensionForce": 0.0,
      "angle": 0.41139972478396003,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -1439.6750951604135,
          -628.125,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "6": {
      "name": "B6",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1686.0454231841584,
      "boltShearForces": [
        1686.0454231841584,
        1686.0454231841584
      ],
      "boltTensionForce": 0.0,
      "angle": 0.3817481468212586,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          1564.675095160413,
          -628.125,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "7": {
      "name": "B7",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 2644.831068020684,
      "boltShearForces": [
        2644.831068020684,
        2644.831068020684
      ],
      "boltTensionForce": 0.0,
      "angle": 0.9951997113820594,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -1439.6750951604135,
          -2218.6633360522023,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "8": {
      "name": "B8",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 2219.5434775516987,
      "boltShearForces": [
        2219.5434775516987,
        2219.5434775516987
      ],
      "boltTensionForce": 0.0,
      "angle": 1.5426336603601973,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          62.49999999999988,
          -2218.6633360522023,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "9": {
      "name": "B9",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 2714.8987369987735,
      "boltShearForces": [
        2714.8987369987735,
        2714.8987369987735
      ],
      "boltTensionForce": 0.0,
      "angle": 0.9565667604180154,
      "fastener_type": "Bolt",
      "member": "B",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          1564.675095160413,
          -2218.6633360522023,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "10": {
      "name": "B10",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1925.1735026034771,
      "boltShearForces": [
        1925.1735026034771,
        1925.1735026034771
      ],
      "boltTensionForce": 0.0,
      "angle": 0.9586231264968182,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          1106.29588091354,
          1575.564165307232,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "11": {
      "name": "B11",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1696.1554924667948,
      "boltShearForces": [
        1696.1554924667948,
        1696.1554924667948
      ],
      "boltTensionForce": 0.0,
      "angle": 1.1914398560259867,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -628.125,
          1575.564165307232,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "12": {
      "name": "B12",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 2839.7227819668965,
      "boltShearForces": [
        2839.7227819668965,
        2839.7227819668965
      ],
      "boltTensionForce": 0.0,
      "angle": 0.5881589440758832,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -2362.54588091354,
          1575.564165307232,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "13": {
      "name": "B13",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1108.0599379664736,
      "boltShearForces": [
        1108.0599379664736,
        1108.0599379664736
      ],
      "boltTensionForce": 0.0,
      "angle": 0.05643484268451593,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          1106.29588091354,
          -62.5,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "15": {
      "name": "B15",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 2363.3724398455556,
      "boltShearForces": [
        2363.3724398455556,
        2363.3724398455556
      ],
      "boltTensionForce": 0.0,
      "angle": 0.026448343965759406,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -2362.54588091354,
          -62.5,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "16": {
      "name": "B16",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 2028.7456855045555,
      "boltShearForces": [
        2028.7456855045555,
        2028.7456855045555
      ],
      "boltTensionForce": 0.0,
      "angle": 0.9940370957366024,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          1106.29588091354,
          -1700.564165307232,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "17": {
      "name": "B17",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 1812.8594804761021,
      "boltShearForces": [
        1812.8594804761021,
        1812.8594804761021
      ],
      "boltTensionForce": 0.0,
      "angle": 1.2169770686321952,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -628.125,
          -1700.564165307232,
          0.0,
          0.0,
          0.0
        ]
      }
    },
    "18": {
      "name": "B18",
      "loadCase": "manual",
      "numberOfShearPlanes": 2,
      "boltAssemblyName": "M12 4.6",
      "boltShearForce": 2910.934818876681,
      "boltShearForces": [
        2910.934818876681,
        2910.934818876681
      ],
      "boltTensionForce": 0.0,
      "angle": 0.62389233783549,
      "fastener_type": "Bolt",
      "member": "C",
      "forcesAllLoadCases": {
        "manual": [
          0.0,
          -2362.54588091354,
          -1700.564165307232,
          0.0,
          0.0,
          0.0
        ]
      }
    }
  },
  "cached_d_mm": 12.0,
  "cached_fub_MPa": 400.0,
  "cached_dowel_strength": {
    "mode": "",
    "product": "",
    "length_mm": 0.0,
    "L_eff_mm": 0.0,
    "p_head_mm": 0.0,
    "M_y_Nm": 0.0,
    "fyb_MPa": 0.0,
    "fub_MPa": 400.0
  },
  "t_steel_idea_extracted_mm": 12.0,
  "outer_plate_y_idea_extracted_mm": 0.0,
  "cached_plate_type": "External",
  "cached_n_inserted_plates": 0,
  "cached_grid_split": 8,
  "cached_member_width_mm": {
    "B": 72.0,
    "C": 72.0
  },
  "cached_member_dims_mm": {
    "B": [
      72.0,
      294.0
    ],
    "C": [
      72.0,
      304.0
    ]
  },
  "cached_member_material_type": {
    "B": "timber",
    "C": "timber"
  },
  "design_exploration_overrides": [],
  "active_dataset": null,
  "semilocked_stash": null,
  "manual_input_model": {
    "scalars": {
      "d_mm": 12.0,
      "bolt_grade": "4.6",
      "t_steel_mm": 12.0,
      "plate_type": "External",
      "substrate_type": "",
      "n_plates": 1,
      "outer_plate_y_mm": 0.0,
      "plate_grade": "S355"
    },
    "members": [
      {
        "name": "B",
        "priority": 1,
        "angle_deg": 0.0,
        "direction_deg": 0,
        "W_mm": 72.0,
        "H_mm": 294.0,
        "timber_class": "C24",
        "t2t_role": "",
        "t2t_role_user_set": false,
        "material": "timber",
        "grain_angle_deg": 0.0,
        "role": "chord*",
        "is_bearing": true,
        "continuous": false,
        "plate_reach_mm": 152.0,
        "plate_offset_mm": 20.0,
        "N_kN": 1.0,
        "Vz_kN": -10.05,
        "My_kNm": 3.25,
        "Vy_kN": 0.0,
        "Mz_kNm": 0.0,
        "T_kNm": 0.0,
        "back_mm": 177.0
      },
      {
        "name": "C",
        "priority": 2,
        "angle_deg": 270.0,
        "direction_deg": 0,
        "W_mm": 72.0,
        "H_mm": 304.0,
        "timber_class": "C24",
        "t2t_role": "",
        "t2t_role_user_set": false,
        "material": "timber",
        "grain_angle_deg": 270.0,
        "role": "brace",
        "is_bearing": false,
        "continuous": false,
        "plate_reach_mm": 441.0,
        "plate_offset_mm": 20.0,
        "N_kN": -10.05,
        "Vz_kN": -1.0,
        "My_kNm": -3.25,
        "Vy_kN": 0.0,
        "Mz_kNm": 0.0,
        "T_kNm": 0.0
      }
    ],
    "grids": [
      {
        "member": "B",
        "type": "Rectangular",
        "rows": 3,
        "cols": 3,
        "s_par_mm": 90.0,
        "s_perp_mm": 85.0,
        "start_offset_mm": 0.0,
        "anchor_perp_mm": 0.0,
        "n_bolts": 6,
        "radius_mm": 80.0,
        "start_angle_deg": 0.0,
        "fastener_type": "Bolt",
        "disabled_indices": [
          4
        ],
        "datum": "node",
        "side": "Forward",
        "row_anchor": "center"
      },
      {
        "member": "C",
        "type": "Rectangular",
        "rows": 3,
        "cols": 3,
        "s_par_mm": 85.0,
        "s_perp_mm": 90.0,
        "start_offset_mm": 62.0,
        "anchor_perp_mm": 0.0,
        "n_bolts": 6,
        "radius_mm": 80.0,
        "start_angle_deg": 0.0,
        "fastener_type": "Bolt",
        "disabled_indices": [
          4
        ],
        "datum": "plate",
        "side": "Forward"
      }
    ],
    "loads_at_node": true
  },
  "cached_bolt_member_map": {
    "1": "B",
    "2": "B",
    "3": "B",
    "4": "B",
    "6": "B",
    "7": "B",
    "8": "B",
    "9": "B",
    "10": "C",
    "11": "C",
    "12": "C",
    "13": "C",
    "15": "C",
    "16": "C",
    "17": "C",
    "18": "C"
  },
  "cached_bolt_iom_index_map": {
    "1": 1,
    "2": 2,
    "3": 3,
    "4": 4,
    "6": 5,
    "7": 6,
    "8": 7,
    "9": 8,
    "10": 9,
    "11": 10,
    "12": 11,
    "13": 12,
    "15": 13,
    "16": 14,
    "17": 15,
    "18": 16
  },
  "cached_iom_bolt_member_map": {
    "0": "B",
    "1": "B",
    "2": "B",
    "3": "B",
    "4": "B",
    "5": "B",
    "6": "B",
    "7": "B",
    "8": "C",
    "9": "C",
    "10": "C",
    "11": "C",
    "12": "C",
    "13": "C",
    "14": "C",
    "15": "C"
  },
  "cached_first_nsp": 2,
  "cached_project_path": "",
  "cached_original_grade": "4.6",
  "cached_original_fastener_type": "Bolt",
  "geometry_data": {
    "beams": [
      {
        "name": "B",
        "id": 0,
        "steel_section_xy_mm": null,
        "steel_rep_plates_3d_mm": null,
        "is_bearing": true,
        "role": "chord*",
        "section_beta_deg": 0.0,
        "grain_dir_3d": [
          1.0,
          0.0,
          0.0
        ],
        "grain_dir_xz": [
          1.0,
          0.0
        ],
        "axis_z_xz": [
          -0.0,
          1.0
        ],
        "xz_polygon_mm": [
          [
            -177.0,
            -147.0
          ],
          [
            400.0,
            -147.0
          ],
          [
            400.0,
            147.0
          ],
          [
            -177.0,
            147.0
          ]
        ],
        "origin_y_mm": 0.0,
        "x_range_mm": [
          -177.0,
          400.0
        ],
        "rep_plate_ids": [],
        "is_continuous": false
      },
      {
        "name": "C",
        "id": 1,
        "steel_section_xy_mm": null,
        "steel_rep_plates_3d_mm": null,
        "is_bearing": false,
        "role": "brace",
        "section_beta_deg": 0.0,
        "grain_dir_3d": [
          -1.8369701987210297e-16,
          0.0,
          -1.0
        ],
        "grain_dir_xz": [
          -1.8369701987210297e-16,
          -1.0
        ],
        "axis_z_xz": [
          1.0,
          -1.8369701987210297e-16
        ],
        "xz_polygon_mm": [
          [
            -152.00000000000003,
            -147.0
          ],
          [
            -152.0000000000001,
            -641.0
          ],
          [
            151.9999999999999,
            -641.0
          ],
          [
            151.99999999999997,
            -147.0
          ]
        ],
        "origin_y_mm": 0.0,
        "x_range_mm": [
          -152.0000000000001,
          151.99999999999997
        ],
        "rep_plate_ids": [],
        "is_continuous": false
      }
    ],
    "plates": [
      {
        "name": "GUSST_1",
        "thickness_mm": 12.0,
        "xz_polygon_mm": [
          [
            131.99999999999997,
            -127.0
          ],
          [
            152.0,
            -127.0
          ],
          [
            152.0,
            127.0
          ],
          [
            -132.0,
            127.0
          ],
          [
            -132.00000000000009,
            -441.0
          ],
          [
            131.99999999999991,
            -441.0
          ]
        ],
        "origin_y_mm": 42.0,
        "x_range_mm": [
          -132.00000000000009,
          152.0
        ]
      },
      {
        "name": "GUSST_2",
        "thickness_mm": 12.0,
        "xz_polygon_mm": [
          [
            131.99999999999997,
            -127.0
          ],
          [
            152.0,
            -127.0
          ],
          [
            152.0,
            127.0
          ],
          [
            -132.0,
            127.0
          ],
          [
            -132.00000000000009,
            -441.0
          ],
          [
            131.99999999999991,
            -441.0
          ]
        ],
        "origin_y_mm": -42.0,
        "x_range_mm": [
          -132.00000000000009,
          152.0
        ]
      }
    ],
    "bolt_grids": [
      {
        "grid_id": 0,
        "bolts": [
          {
            "bolt_index": 1,
            "xz_mm": [
              -90.0,
              -85.0
            ]
          },
          {
            "bolt_index": 2,
            "xz_mm": [
              -90.0,
              0.0
            ]
          },
          {
            "bolt_index": 3,
            "xz_mm": [
              -90.0,
              85.0
            ]
          },
          {
            "bolt_index": 4,
            "xz_mm": [
              0.0,
              -85.0
            ]
          },
          {
            "bolt_index": 5,
            "xz_mm": [
              0.0,
              85.0
            ]
          },
          {
            "bolt_index": 6,
            "xz_mm": [
              90.0,
              -85.0
            ]
          },
          {
            "bolt_index": 7,
            "xz_mm": [
              90.0,
              0.0
            ]
          },
          {
            "bolt_index": 8,
            "xz_mm": [
              90.0,
              85.0
            ]
          }
        ],
        "axis_x_3d": [
          1.0,
          0.0,
          0.0
        ],
        "axis_y_3d": [
          -0.0,
          0.0,
          1.0
        ],
        "connected_parts": [
          0
        ]
      },
      {
        "grid_id": 1,
        "bolts": [
          {
            "bolt_index": 9,
            "xz_mm": [
              -90.00000000000007,
              -379.0
            ]
          },
          {
            "bolt_index": 10,
            "xz_mm": [
              -6.962117053152702e-14,
              -379.0
            ]
          },
          {
            "bolt_index": 11,
            "xz_mm": [
              89.99999999999993,
              -379.0
            ]
          },
          {
            "bolt_index": 12,
            "xz_mm": [
              -90.00000000000006,
              -294.0
            ]
          },
          {
            "bolt_index": 13,
            "xz_mm": [
              89.99999999999994,
              -294.0
            ]
          },
          {
            "bolt_index": 14,
            "xz_mm": [
              -90.00000000000004,
              -208.99999999999997
            ]
          },
          {
            "bolt_index": 15,
            "xz_mm": [
              -3.839267715326952e-14,
              -209.0
            ]
          },
          {
            "bolt_index": 16,
            "xz_mm": [
              89.99999999999996,
              -209.00000000000003
            ]
          }
        ],
        "axis_x_3d": [
          -1.8369701987210297e-16,
          0.0,
          -1.0
        ],
        "axis_y_3d": [
          1.0,
          0.0,
          -1.8369701987210297e-16
        ],
        "connected_parts": [
          1
        ]
      }
    ],
    "all_bolts": [
      {
        "bolt_index": 1,
        "stable_id": 1,
        "xz_mm": [
          -90.0,
          -85.0
        ],
        "xy_mm": [
          -90.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 2,
        "stable_id": 2,
        "xz_mm": [
          -90.0,
          0.0
        ],
        "xy_mm": [
          -90.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 3,
        "stable_id": 3,
        "xz_mm": [
          -90.0,
          85.0
        ],
        "xy_mm": [
          -90.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 4,
        "stable_id": 4,
        "xz_mm": [
          0.0,
          -85.0
        ],
        "xy_mm": [
          0.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 5,
        "stable_id": 6,
        "xz_mm": [
          0.0,
          85.0
        ],
        "xy_mm": [
          0.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 6,
        "stable_id": 7,
        "xz_mm": [
          90.0,
          -85.0
        ],
        "xy_mm": [
          90.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 7,
        "stable_id": 8,
        "xz_mm": [
          90.0,
          0.0
        ],
        "xy_mm": [
          90.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 8,
        "stable_id": 9,
        "xz_mm": [
          90.0,
          85.0
        ],
        "xy_mm": [
          90.0,
          0.0
        ],
        "grid_seq": 0,
        "grid_type": "Rectangular",
        "member_name": "B",
        "member_role": "chord*",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 9,
        "stable_id": 10,
        "xz_mm": [
          -90.00000000000007,
          -379.0
        ],
        "xy_mm": [
          -90.00000000000007,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 10,
        "stable_id": 11,
        "xz_mm": [
          -6.962117053152702e-14,
          -379.0
        ],
        "xy_mm": [
          -6.962117053152702e-14,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 11,
        "stable_id": 12,
        "xz_mm": [
          89.99999999999993,
          -379.0
        ],
        "xy_mm": [
          89.99999999999993,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 12,
        "stable_id": 13,
        "xz_mm": [
          -90.00000000000006,
          -294.0
        ],
        "xy_mm": [
          -90.00000000000006,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 13,
        "stable_id": 15,
        "xz_mm": [
          89.99999999999994,
          -294.0
        ],
        "xy_mm": [
          89.99999999999994,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 14,
        "stable_id": 16,
        "xz_mm": [
          -90.00000000000004,
          -208.99999999999997
        ],
        "xy_mm": [
          -90.00000000000004,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 15,
        "stable_id": 17,
        "xz_mm": [
          -3.839267715326952e-14,
          -209.0
        ],
        "xy_mm": [
          -3.839267715326952e-14,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      },
      {
        "bolt_index": 16,
        "stable_id": 18,
        "xz_mm": [
          89.99999999999996,
          -209.00000000000003
        ],
        "xy_mm": [
          89.99999999999996,
          0.0
        ],
        "grid_seq": 1,
        "grid_type": "Rectangular",
        "member_name": "C",
        "member_role": "brace",
        "corner_bolt_swap": false,
        "export_fastener_type": "Bolt",
        "corner_bolt_grade": null,
        "corner_bolt_source": null,
        "corner_bolt_reason": null,
        "corner_bolt_option": null,
        "corner_bolt_oversize_mm": null,
        "calculation_fastener_type": "Bolt",
        "dowel_catalog": null
      }
    ],
    "disabled_bolts": [
      {
        "stable_id": 5,
        "xz_mm": [
          0.0,
          0.0
        ],
        "xy_mm": [
          0.0,
          0.0
        ],
        "member": "B",
        "grid_seq": 0,
        "auto_disabled": false,
        "reason": "manually disabled"
      },
      {
        "stable_id": 14,
        "xz_mm": [
          -5.400692384239827e-14,
          -294.0
        ],
        "xy_mm": [
          -5.400692384239827e-14,
          0.0
        ],
        "member": "C",
        "grid_seq": 1,
        "auto_disabled": false,
        "reason": "manually disabled"
      }
    ]
  },
  "cached_tekla_plates": [
    {
      "global_polygon_m": [
        [
          0.13199999999999998,
          0.042,
          -0.127
        ],
        [
          0.152,
          0.042,
          -0.127
        ],
        [
          0.152,
          0.042,
          0.127
        ],
        [
          -0.132,
          0.042,
          0.127
        ],
        [
          -0.1320000000000001,
          0.042,
          -0.441
        ],
        [
          0.13199999999999992,
          0.042,
          -0.441
        ]
      ],
      "thickness_m": 0.012,
      "material": "S355",
      "name": "GUSST_1",
      "normal": [
        0.0,
        1.0,
        0.0
      ],
      "_baseline_centroid_proj_m": 0.042
    },
    {
      "global_polygon_m": [
        [
          0.13199999999999998,
          -0.042,
          -0.127
        ],
        [
          0.152,
          -0.042,
          -0.127
        ],
        [
          0.152,
          -0.042,
          0.127
        ],
        [
          -0.132,
          -0.042,
          0.127
        ],
        [
          -0.1320000000000001,
          -0.042,
          -0.441
        ],
        [
          0.13199999999999992,
          -0.042,
          -0.441
        ]
      ],
      "thickness_m": 0.012,
      "material": "S355",
      "name": "GUSST_2",
      "normal": [
        0.0,
        1.0,
        0.0
      ],
      "_baseline_centroid_proj_m": -0.042
    }
  ],
  "cached_tekla_bolts": [
    {
      "position_m": [
        -0.09,
        0.0,
        -0.085
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        -0.09,
        0.0,
        0.0
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        -0.09,
        0.0,
        0.085
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.0,
        0.0,
        -0.085
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.0,
        0.0,
        0.085
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.09,
        0.0,
        -0.085
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.09,
        0.0,
        0.0
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.09,
        0.0,
        0.085
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 0,
      "connected_parts": [
        0
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        -0.09000000000000007,
        0.0,
        -0.379
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        -6.962117053152702e-17,
        0.0,
        -0.379
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.08999999999999993,
        0.0,
        -0.379
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        -0.09000000000000005,
        0.0,
        -0.294
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.08999999999999994,
        0.0,
        -0.294
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        -0.09000000000000004,
        0.0,
        -0.20899999999999996
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        -3.839267715326952e-17,
        0.0,
        -0.209
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    },
    {
      "position_m": [
        0.08999999999999996,
        0.0,
        -0.20900000000000002
      ],
      "diameter_mm": 12.0,
      "grade": "4.6",
      "grid_id": 1,
      "connected_parts": [
        1
      ],
      "axis": [
        0.0,
        1.0,
        0.0
      ],
      "corner_bolt_swap": false,
      "export_fastener_type": "Bolt",
      "corner_bolt_grade": null,
      "corner_bolt_source": null,
      "corner_bolt_reason": null,
      "calculation_fastener_type": "Bolt",
      "dowel_catalog": null
    }
  ],
  "cached_tekla_bearing_dir": [
    1.0,
    0.0
  ],
  "cached_iom_beam_axes": {
    "0": [
      1.0,
      0.0,
      0.0
    ],
    "1": [
      -1.8369701987210297e-16,
      0.0,
      -1.0
    ]
  },
  "cached_member_outlines": [
    {
      "name": "B",
      "id": 0,
      "polygon_3d_m": [
        [
          -0.177,
          0.0,
          -0.147
        ],
        [
          0.4,
          0.0,
          -0.147
        ],
        [
          0.4,
          0.0,
          0.147
        ],
        [
          -0.177,
          0.0,
          0.147
        ]
      ],
      "axis": [
        1.0,
        0.0,
        0.0
      ],
      "origin_m": [
        0.0,
        0.0,
        0.0
      ],
      "axis_x": [
        1.0,
        0.0,
        0.0
      ],
      "axis_y": [
        0.0,
        1.0,
        0.0
      ],
      "axis_z": [
        -0.0,
        0.0,
        1.0
      ],
      "x_range_m": [
        -0.177,
        0.4
      ],
      "depth_m": 0.294,
      "width_mm": 72.0,
      "grade": "C24",
      "material_type": "timber"
    },
    {
      "name": "C",
      "id": 1,
      "polygon_3d_m": [
        [
          -0.15200000000000002,
          0.0,
          -0.147
        ],
        [
          -0.1520000000000001,
          0.0,
          -0.641
        ],
        [
          0.15199999999999989,
          0.0,
          -0.641
        ],
        [
          0.15199999999999997,
          0.0,
          -0.147
        ]
      ],
      "axis": [
        -1.8369701987210297e-16,
        0.0,
        -1.0
      ],
      "origin_m": [
        0.0,
        0.0,
        0.0
      ],
      "axis_x": [
        -1.8369701987210297e-16,
        0.0,
        -1.0
      ],
      "axis_y": [
        0.0,
        1.0,
        0.0
      ],
      "axis_z": [
        1.0,
        0.0,
        -1.8369701987210297e-16
      ],
      "x_range_m": [
        0.14699999999999996,
        0.641
      ],
      "depth_m": 0.304,
      "width_mm": 72.0,
      "grade": "C24",
      "material_type": "timber"
    }
  ],
  "tekla_export_settings": {
    "dowel_name": "DOWEL",
    "dowel_class": "101",
    "dowel_pt_prefix": "",
    "dowel_pt_start": "1",
    "dowel_as_prefix": "",
    "dowel_as_start": "1",
    "dowel_tol_timber": 0.0,
    "dowel_tol_steel": 0.0,
    "dowel_cut_timber": true,
    "dowel_cut_steel": true,
    "nail_name": "NAIL",
    "nail_class": "102",
    "nail_pt_prefix": "",
    "nail_pt_start": "1",
    "nail_as_prefix": "",
    "nail_as_start": "1",
    "nail_tol_timber": 0.0,
    "nail_tol_steel": 0.0,
    "nail_cut_timber": true,
    "nail_cut_steel": true,
    "screw_name": "SCREW",
    "screw_class": "102",
    "screw_pt_prefix": "",
    "screw_pt_start": "1",
    "screw_as_prefix": "",
    "screw_as_start": "1",
    "screw_tol_timber": 0.0,
    "screw_tol_steel": 0.0,
    "screw_cut_timber": true,
    "screw_cut_steel": true,
    "bolt_standard": "931",
    "bolt_tolerance": 0.0,
    "bolt_rotation": "TOP",
    "bolt_recess_cut_timber": true,
    "slot_width_tol": 0.0,
    "slot_end_offset": 10.0,
    "hole_oversize_plate": 0.0,
    "recess_washer_delta": 0.0,
    "flip_after_export": false
  },
  "cached_member_info": [
    {
      "id": 0,
      "name": "B",
      "is_bearing": true,
      "beta_rad": 0.0
    },
    {
      "id": 1,
      "name": "C",
      "is_bearing": false,
      "beta_rad": -1.5707963267948968
    }
  ],
  "force_decomposition": {
    "active_lc": "manual",
    "per_member": {
      "B": {
        "V_net_xz_N": [
          499.9999999999982,
          -5025.0
        ],
        "V_net_magnitude_N": 5049.814353023287,
        "sum_F_total_N": 15369.194628475569,
        "tau": 0.3285672720720933,
        "classification": "rotational",
        "alpha_rad": 1.471620285101327,
        "V_perp_N": 5025.0,
        "bolt_count": 8
      },
      "C": {
        "V_net_xz_N": [
          -499.9999999999993,
          5024.999999999999
        ],
        "V_net_magnitude_N": 5049.8143530232865,
        "sum_F_total_N": 16685.024139706533,
        "tau": 0.30265550176855216,
        "classification": "rotational",
        "alpha_rad": 0.0991760416935702,
        "V_perp_N": 500.00000000000017,
        "bolt_count": 8
      }
    },
    "per_bolt_Fxz_N": {
      "1": [
        -1439.6750951604135,
        962.4133360522023
      ],
      "2": [
        62.49999999999988,
        962.4133360522023
      ],
      "3": [
        1564.675095160413,
        962.4133360522023
      ],
      "4": [
        -1439.6750951604135,
        -628.125
      ],
      "6": [
        1564.675095160413,
        -628.125
      ],
      "7": [
        -1439.6750951604135,
        -2218.6633360522023
      ],
      "8": [
        62.49999999999988,
        -2218.6633360522023
      ],
      "9": [
        1564.675095160413,
        -2218.6633360522023
      ],
      "10": [
        1575.5641653072319,
        -1106.2958809135403
      ],
      "11": [
        1575.5641653072323,
        628.1249999999997
      ],
      "12": [
        1575.5641653072325,
        2362.5458809135393
      ],
      "13": [
        -62.500000000000206,
        -1106.29588091354
      ],
      "15": [
        -62.49999999999957,
        2362.54588091354
      ],
      "16": [
        -1700.5641653072323,
        -1106.2958809135398
      ],
      "17": [
        -1700.5641653072319,
        628.1250000000003
      ],
      "18": [
        -1700.5641653072316,
        2362.5458809135403
      ]
    },
    "per_bolt_member": {
      "1": "B",
      "2": "B",
      "3": "B",
      "4": "B",
      "6": "B",
      "7": "B",
      "8": "B",
      "9": "B",
      "10": "C",
      "11": "C",
      "12": "C",
      "13": "C",
      "15": "C",
      "16": "C",
      "17": "C",
      "18": "C"
    },
    "bolt_key_to_seq": {
      "1": 0,
      "2": 1,
      "3": 2,
      "4": 3,
      "6": 4,
      "7": 5,
      "8": 6,
      "9": 7,
      "10": 8,
      "11": 9,
      "12": 10,
      "13": 11,
      "15": 12,
      "16": 13,
      "17": 14,
      "18": 15
    }
  },
  "member_forces": {
    "active_lc": "manual",
    "members": {
      "B": {
        "N_kN": 1.0,
        "N_net_kN": 1.0,
        "N_begin_kN": 1.0,
        "N_end_kN": 1.0,
        "t2t_mirror_scale": 1.0,
        "is_continuous": false,
        "is_tension": true,
        "is_bearing": true,
        "position": "End",
        "Vz_kN": -10.05,
        "Vz_begin_kN": -10.05,
        "Vz_end_kN": -10.05,
        "Vy_kN": 0.0,
        "Mx_kNm": 0.0,
        "My_kNm": 3.25,
        "Mz_kNm": 0.0,
        "sides": [
          {
            "position": "End",
            "N_kN": 1.0,
            "Vz_kN": -10.05,
            "Vy_kN": 0.0,
            "Mx_kNm": 0.0,
            "My_kNm": 3.25,
            "Mz_kNm": 0.0,
            "is_tension": true
          }
        ]
      },
      "C": {
        "N_kN": -10.05,
        "N_net_kN": 10.05,
        "N_begin_kN": -10.05,
        "N_end_kN": -10.05,
        "t2t_mirror_scale": 1.0,
        "is_continuous": false,
        "is_tension": false,
        "is_bearing": false,
        "position": "End",
        "Vz_kN": -1.0,
        "Vz_begin_kN": -1.0,
        "Vz_end_kN": -1.0,
        "Vy_kN": 0.0,
        "Mx_kNm": 0.0,
        "My_kNm": -3.25,
        "Mz_kNm": 0.0,
        "sides": [
          {
            "position": "End",
            "N_kN": -10.05,
            "Vz_kN": -1.0,
            "Vy_kN": 0.0,
            "Mx_kNm": 0.0,
            "My_kNm": -3.25,
            "Mz_kNm": 0.0,
            "is_tension": false
          }
        ]
      }
    }
  },
  "n_ef_results": {
    "B": {
      "n_total": 8,
      "n_rows": 0,
      "n_per_row": [],
      "a1_mm": null,
      "a1_per_row": [],
      "alpha_deg": 84.31763138214495,
      "alpha_rad": 1.4716202851013265,
      "n_ef": 8.0,
      "n_ef_total": 8.0,
      "n_ef_per_row": [],
      "n_ef_0_per_row": [],
      "n_ef_pre_override_per_row": [],
      "n_ef_pre_override_total": 8.0,
      "n_ef_reduction_disabled": false,
      "n_ef_override_reason": "",
      "reason": "rotational (τ=0.33 < 0.40)",
      "d_mm": 12.0,
      "tau": 0.3286,
      "N_kN": 1.0,
      "Vz_kN": -10.05,
      "F_v_Rd_min_ec5_kN": 9.876551743553081,
      "F_v_Rd_min_fprEN_kN": 12.345689679441351,
      "F_v_Rk_min_ec5_kN": 14.26613029624334,
      "F_v_Rk_min_fprEN_kN": 17.832662870304176,
      "F_v_p_Rk_jhs_min_ec5_kN": null,
      "F_v_p_Rk_jhs_min_fprEN_kN": null,
      "n_plates": 0,
      "k_mod": 0.9,
      "gamma_M": 1.3,
      "mode_compatible_member": true,
      "partial_incompat_member": false,
      "n_bolts_in_member": 8,
      "n_bolts_incompat": 0,
      "V_Ed_at_gov_plane_sum_kN": 15.369194628475569,
      "F_v_Rk_per_plane_gov_min_ec5_kN": 7.13306514812167,
      "F_v_Rk_per_plane_gov_min_fprEN_kN": 8.916331435152088,
      "F_v_Rd_per_plane_gov_min_ec5_kN": 4.938275871776541,
      "F_v_Rd_per_plane_gov_min_fprEN_kN": 6.172844839720676,
      "V_Ed_member_kN": 1.0,
      "nef_routing": "bolt -> 8.5.1.1(4)"
    },
    "C": {
      "n_total": 8,
      "n_rows": 0,
      "n_per_row": [],
      "a1_mm": null,
      "a1_per_row": [],
      "alpha_deg": 5.6823686178550545,
      "alpha_rad": 0.09917604169357014,
      "n_ef": 8.0,
      "n_ef_total": 8.0,
      "n_ef_per_row": [],
      "n_ef_0_per_row": [],
      "n_ef_pre_override_per_row": [],
      "n_ef_pre_override_total": 8.0,
      "n_ef_reduction_disabled": false,
      "n_ef_override_reason": "",
      "reason": "rotational (τ=0.30 < 0.40)",
      "d_mm": 12.0,
      "tau": 0.3027,
      "N_kN": -10.05,
      "Vz_kN": -1.0,
      "F_v_Rd_min_ec5_kN": 10.302270273487041,
      "F_v_Rd_min_fprEN_kN": 12.877837841858803,
      "F_v_Rk_min_ec5_kN": 14.881057061703505,
      "F_v_Rk_min_fprEN_kN": 18.60132132712938,
      "F_v_p_Rk_jhs_min_ec5_kN": null,
      "F_v_p_Rk_jhs_min_fprEN_kN": null,
      "n_plates": 0,
      "k_mod": 0.9,
      "gamma_M": 1.3,
      "mode_compatible_member": true,
      "partial_incompat_member": false,
      "n_bolts_in_member": 8,
      "n_bolts_incompat": 0,
      "V_Ed_at_gov_plane_sum_kN": 16.685024139706535,
      "F_v_Rk_per_plane_gov_min_ec5_kN": 7.440528530851752,
      "F_v_Rk_per_plane_gov_min_fprEN_kN": 9.30066066356469,
      "F_v_Rd_per_plane_gov_min_ec5_kN": 5.1511351367435205,
      "F_v_Rd_per_plane_gov_min_fprEN_kN": 6.438918920929401,
      "V_Ed_member_kN": 10.05,
      "nef_routing": "bolt -> 8.5.1.1(4)"
    }
  },
  "block_shear_results": {
    "B": {
      "skip": "rotational (τ=0.3286 < τ_min=0.40)",
      "regime": "rotational",
      "tau": 0.3286,
      "tau_min": 0.4,
      "N_kN": 1.0
    },
    "C": {
      "skip": "compression",
      "N_kN": -10.1
    }
  },
  "member_net_section_results": {
    "B": {
      "member_name": "B",
      "w_width_mm": 72.0,
      "h_depth_mm": 294.0,
      "d0_mm": 12.0,
      "n_holes": 3,
      "timber_class": "C24",
      "k_mod": 0.9,
      "gamma_M": 1.3,
      "k_sys": 1.0,
      "skip": null,
      "notes": [],
      "b_net_mm": 72.0,
      "d0_oversize_mm": 0.0,
      "N_Ed_kN": 1.0,
      "check_type": "tension",
      "clause": "EN 1995-1-1 6.1.2",
      "section_holes_z_mm": [
        -85.0,
        0.0,
        85.0
      ],
      "A_gross_mm2": 21168.0,
      "A_holes_mm2": 2592.0,
      "A_net_mm2": 18576.0,
      "area_used_mm2": 18576.0,
      "used_gross": false,
      "f_k_MPa": 14.0,
      "k_h": 1.0,
      "k_h_applies": false,
      "k_h_basis": "solid, max dim >= 150 mm (no increase)",
      "f_d_MPa": 9.6923,
      "sigma_d_MPa": 0.0538,
      "eta_axial": 0.0056,
      "governing_check": "EN 1995-1-1 6.1.7 (net shear)",
      "My_kNm": 3.25,
      "Vz_kN": -10.05,
      "V_dw_kN": 9.5432,
      "S_net_mm3": 704484.0,
      "I_net_mm4": 139957200.0,
      "z_s_mm": 147.0,
      "f_m_k_MPa": 24.0,
      "k_h_bending": 1.0,
      "k_h_bending_applies": false,
      "k_h_bending_basis": "solid, max dim >= 150 mm (no increase)",
      "f_m_d_MPa": 16.6154,
      "sigma_m_MPa": 3.4135,
      "eta_NM": 0.211,
      "f_v_k_MPa": 4.0,
      "f_v_d_MPa": 2.7692,
      "k_cr": 0.67,
      "tau_v_MPa": 1.0487,
      "tau_dw_MPa": 0.9958,
      "eta_shear_v": 0.3787,
      "eta_shear_dw": 0.3596,
      "eta": 0.3787,
      "status": "PASS",
      "section_selection_requested": "automatic",
      "section_selection_effective": "automatic",
      "section_selection_fallback_reason": null,
      "crit_section_xz": [
        [
          90.0,
          -147.0
        ],
        [
          90.0,
          147.0
        ]
      ],
      "crit_holes_xz": [],
      "crit_holes_bids": [],
      "crit_holes_r_mm": 10.0,
      "crit_station_mm": 90.0
    },
    "C": {
      "member_name": "C",
      "w_width_mm": 72.0,
      "h_depth_mm": 304.0,
      "d0_mm": 12.0,
      "n_holes": 3,
      "timber_class": "C24",
      "k_mod": 0.9,
      "gamma_M": 1.3,
      "k_sys": 1.0,
      "skip": null,
      "notes": [
        "section squash only (6.1.4); member stability (6.3) checked separately"
      ],
      "b_net_mm": 72.0,
      "d0_oversize_mm": 0.0,
      "N_Ed_kN": -10.05,
      "check_type": "compression",
      "clause": "EN 1995-1-1 6.1.4",
      "section_holes_z_mm": [
        -90.0,
        0.0,
        90.0
      ],
      "A_gross_mm2": 21888.0,
      "A_holes_mm2": 2592.0,
      "A_net_mm2": 19296.0,
      "area_used_mm2": 19296.0,
      "used_gross": false,
      "f_k_MPa": 21.0,
      "k_h": 1.0,
      "k_h_applies": false,
      "k_h_basis": "compression: k_h not applicable",
      "f_d_MPa": 14.5385,
      "sigma_d_MPa": 0.5208,
      "eta_axial": 0.0358,
      "governing_check": "EN 1995-1-1 6.1.7 (moment-induced V_dw)",
      "My_kNm": -3.25,
      "Vz_kN": -1.0,
      "V_dw_kN": 9.0131,
      "S_net_mm3": 753984.0,
      "I_net_mm4": 154538880.0,
      "z_s_mm": 152.0,
      "f_m_k_MPa": 24.0,
      "k_h_bending": 1.0,
      "k_h_bending_applies": false,
      "k_h_bending_basis": "solid, max dim >= 150 mm (no increase)",
      "f_m_d_MPa": 16.6154,
      "sigma_m_MPa": 3.1966,
      "eta_NM": 0.1937,
      "f_v_k_MPa": 4.0,
      "f_v_d_MPa": 2.7692,
      "k_cr": 0.67,
      "tau_v_MPa": 0.1011,
      "tau_dw_MPa": 0.9116,
      "eta_shear_v": 0.0365,
      "eta_shear_dw": 0.3292,
      "eta": 0.3292,
      "status": "PASS",
      "section_selection_requested": "automatic",
      "section_selection_effective": "automatic",
      "section_selection_fallback_reason": null,
      "crit_section_xz": [
        [
          -152.00000000000006,
          -379.0
        ],
        [
          151.99999999999994,
          -379.0
        ]
      ],
      "crit_holes_xz": [],
      "crit_holes_bids": [],
      "crit_holes_r_mm": 10.0,
      "crit_station_mm": 379.0
    }
  },
  "heimeshoff_ring_shear_result": {
    "requested": false,
    "effective": false,
    "eligible": false,
    "eligibility_reason": "Requires a timber-to-timber connection.",
    "ring_center_xz_mm": null,
    "rings": [],
    "S_r_mm": null,
    "I_p_mm2": null,
    "members": {},
    "governing_member": null,
    "eta": null,
    "status": "N/A"
  },
  "splitting_results": {
    "B": {
      "skip": "auto: rotational (tau=0.3286 < tau_min=0.40)",
      "regime": "rotational",
      "member_name": "B",
      "tau": 0.3286,
      "tau_min": 0.4,
      "eta": 0.0,
      "status": "N/A"
    },
    "C": {
      "skip": "auto: rotational (tau=0.3027 < tau_min=0.40)",
      "regime": "rotational",
      "member_name": "C",
      "tau": 0.3027,
      "tau_min": 0.4,
      "eta": 0.0,
      "status": "N/A"
    }
  },
  "spacing_results": {
    "B": {
      "alpha_deg": 275.68236861785505,
      "n_bolts": 8,
      "n_rows": 3,
      "d_mm": 12.0,
      "a1_actual_mm": 90.0,
      "a1_required_mm": 49.188162490846395,
      "a2_actual_mm": 85.0,
      "a2_required_mm": 48.0,
      "a3t_actual_mm": 87.0,
      "a3t_required_mm": null,
      "a3c_actual_mm": 87.0,
      "a3c_required_mm": 48.0,
      "a4t_actual_mm": 62.0,
      "a4t_required_mm": 47.88206606601244,
      "a4c_actual_mm": 62.0,
      "a4c_required_mm": 36.0,
      "table": "8.4",
      "spacing_formula_basis": {
        "schema": 1,
        "table": "8.4",
        "rules": {
          "a1": {
            "kind": "table",
            "applied_rule": "a1",
            "base_required_mm": 49.188162490846395,
            "final_required_mm": 49.188162490846395,
            "fire_increment_mm": 0.0
          },
          "a2": {
            "kind": "table",
            "applied_rule": "a2",
            "base_required_mm": 48.0,
            "final_required_mm": 48.0,
            "fire_increment_mm": 0.0
          },
          "a3,t": {
            "kind": "table",
            "applied_rule": "a3,t",
            "base_required_mm": null,
            "final_required_mm": null,
            "fire_increment_mm": 0.0
          },
          "a3,c": {
            "kind": "rotational_floor",
            "applied_rule": "a3,c",
            "lookup_alpha_deg": 180.0,
            "base_required_mm": 48.0,
            "final_required_mm": 48.0,
            "fire_increment_mm": 0.0
          },
          "a4,t": {
            "kind": "table",
            "applied_rule": "a4,t",
            "base_required_mm": 47.88206606601244,
            "final_required_mm": 47.88206606601244,
            "fire_increment_mm": 0.0
          },
          "a4,c": {
            "kind": "table",
            "applied_rule": "a4,c",
            "base_required_mm": 36.0,
            "final_required_mm": 36.0,
            "fire_increment_mm": 0.0
          }
        }
      },
      "a4t_on_positive_perp": true,
      "loaded_edge_indeterminate": false,
      "a4t_rule_key": "a4,t",
      "a4c_rule_key": "a4,c",
      "a4t_face": "Depth+",
      "a4c_face": "Depth-",
      "loaded_edge_signal_kN": -10.05,
      "loaded_edge_beta_flip": 1.0,
      "loaded_edge_beta_source": "beta",
      "a_fi_mm": 0.0,
      "fire_a3_multiplier": 1.0,
      "end_exposed": true,
      "a4t_face_exposed": true,
      "a4c_face_exposed": true,
      "fire_surcharge_waived_mm": {
        "a3": 0.0,
        "a4t": 0.0,
        "a4c": 0.0
      },
      "violations": [],
      "status": "PASS",
      "loaded_end_indeterminate": false
    },
    "C": {
      "alpha_deg": 185.68236861785505,
      "n_bolts": 8,
      "n_rows": 3,
      "d_mm": 12.0,
      "a1_actual_mm": 85.0,
      "a1_required_mm": 59.94103303300622,
      "a2_actual_mm": 90.0,
      "a2_required_mm": 48.0,
      "a3t_actual_mm": 61.99999999999998,
      "a3t_required_mm": null,
      "a3c_actual_mm": 61.99999999999998,
      "a3c_required_mm": 48.0,
      "a4t_actual_mm": 62.0,
      "a4t_required_mm": 36.0,
      "a4c_actual_mm": 61.99999999999999,
      "a4c_required_mm": 36.0,
      "table": "8.4",
      "spacing_formula_basis": {
        "schema": 1,
        "table": "8.4",
        "rules": {
          "a1": {
            "kind": "table",
            "applied_rule": "a1",
            "base_required_mm": 59.94103303300622,
            "final_required_mm": 59.94103303300622,
            "fire_increment_mm": 0.0
          },
          "a2": {
            "kind": "table",
            "applied_rule": "a2",
            "base_required_mm": 48.0,
            "final_required_mm": 48.0,
            "fire_increment_mm": 0.0
          },
          "a3,t": {
            "kind": "table",
            "applied_rule": "a3,t",
            "base_required_mm": null,
            "final_required_mm": null,
            "fire_increment_mm": 0.0
          },
          "a3,c": {
            "kind": "rotational_floor",
            "applied_rule": "a3,c",
            "lookup_alpha_deg": 180.0,
            "base_required_mm": 48.0,
            "final_required_mm": 48.0,
            "fire_increment_mm": 0.0
          },
          "a4,t": {
            "kind": "table",
            "applied_rule": "a4,t",
            "base_required_mm": 36.0,
            "final_required_mm": 36.0,
            "fire_increment_mm": 0.0
          },
          "a4,c": {
            "kind": "table",
            "applied_rule": "a4,c",
            "base_required_mm": 36.0,
            "final_required_mm": 36.0,
            "fire_increment_mm": 0.0
          }
        }
      },
      "a4t_on_positive_perp": true,
      "loaded_edge_indeterminate": false,
      "a4t_rule_key": "a4,t",
      "a4c_rule_key": "a4,c",
      "a4t_face": "Depth+",
      "a4c_face": "Depth-",
      "loaded_edge_signal_kN": -1.0,
      "loaded_edge_beta_flip": 1.0,
      "loaded_edge_beta_source": "beta",
      "a_fi_mm": 0.0,
      "fire_a3_multiplier": 1.0,
      "end_exposed": true,
      "a4t_face_exposed": true,
      "a4c_face_exposed": true,
      "fire_surcharge_waived_mm": {
        "a3": 0.0,
        "a4t": 0.0,
        "a4c": 0.0
      },
      "violations": [],
      "status": "PASS",
      "loaded_end_indeterminate": false
    }
  },
  "fire_results": null,
  "calc_settings": {
    "tau_min": 0.4,
    "Vz_min_kN": 0.1,
    "hole_oversize_bolt": 0.0,
    "hole_oversize_dowel": 0.0,
    "gamma_M_solid": 1.3,
    "gamma_M_glulam": 1.25,
    "gamma_M_panel": 1.2,
    "gamma_M2": 1.25,
    "threads_in_shear": true,
    "k_cr": 0.67,
    "a1_sum": false,
    "plug_shear": true,
    "force_net_section_at_node": false,
    "use_heimeshoff_ring_shear": false
  },
  "pdf_export_settings": {
    "project_name": "",
    "project_number": "",
    "project_address": "",
    "engineer_name": "",
    "checked_by": "",
    "report_date": "",
    "company_logo_b64": "",
    "output_folder": "",
    "output_filename": "",
    "include_view_xz": true,
    "include_view_yz": true,
    "include_view_xy": true,
    "include_force_vectors": true,
    "include_derivations": true,
    "include_embodied_carbon": true,
    "include_spacing": true,
    "pdf_bolt_johansen_mode": "governing",
    "pdf_bolt_johansen_bolt": "",
    "include_fprEN_table": true,
    "include_bolt_johansen_fprEN": false,
    "epd_factor": 1.55,
    "pdf_language": "en"
  },
  "step_export_settings": {
    "include_node_marker": true,
    "include_members": true,
    "include_plates": true,
    "include_fasteners": true,
    "include_recesses": true,
    "cut_steel_plates": true,
    "cut_members": true,
    "single_plate_to_xy": false
  },
  "ifc_export_settings": {
    "include_node_marker": true,
    "timber_transparency": 0.0
  },
  "dxf_export_settings": {
    "view_xz": true,
    "view_xy": true
  },
  "ui_timber_class": "C24",
  "ui_service_class": "1",
  "ui_load_duration": "Short-term",
  "ui_fastener_type": "Bolt",
  "ui_nail_length_mm": 0.0,
  "ui_rope_effect": true,
  "ui_force_net_section_at_node": false,
  "ui_heimeshoff_ring_shear": false,
  "ui_splitting_overrides": {},
  "ui_n_ef_overrides": {},
  "ui_Vz_min_kN": "0.10",
  "ui_a1_sum": false,
  "ui_show_block_shear": true,
  "ui_show_force_arrows": true,
  "ui_show_bolt_eta": true,
  "ui_show_member_labels": true,
  "ui_show_spacing_zones": true,
  "ui_show_spacing_zone_inner": true,
  "ui_show_spacing_zone_outer1": true,
  "ui_show_spacing_zone_outer2": true,
  "ui_show_plane_force": true,
  "ui_show_net_section": true,
  "ui_show_depth_axis": true,
  "ui_view3d": {
    "mode": "solid",
    "translucent": false,
    "node_axes": true,
    "zones_on": true,
    "force_vectors": false,
    "block_shear": false,
    "net_section": false,
    "bearing": false,
    "hidden": []
  },
  "ui_fastener_grade": "4.6",
  "ui_dowel_offset": "0",
  "ui_countersink_by_member": {},
  "ui_dowel_head_insertion_p": "0",
  "ui_slot_tol": "0",
  "ui_a3_delta": "0",
  "ui_t_steel_actual": "12.00",
  "ui_outer_plate_y_actual": "0",
  "ui_diameter": "12",
  "ui_washer_diameter": "36",
  "ui_fyk_custom": "240",
  "ui_fuk_custom": "400",
  "ui_fire_class": "None",
  "ui_eta_fi": "0.60",
  "ui_fire_regime": "Auto",
  "ui_fire_cover_afi": "0",
  "ui_fire_hp": "0",
  "ui_fire_board_hp": "0",
  "ui_fire_dowel_flush": true,
  "ui_fire_exposed_faces": {},
  "ui_plate_grade": "S355",
  "ui_tau_min": "0.40",
  "ui_hole_oversize_bolt": "0.0",
  "ui_hole_oversize_dowel": "0.0",
  "ui_gamma_M_solid": "1.30",
  "ui_gamma_M_glulam": "1.25",
  "ui_gamma_M_panel": "1.20",
  "ui_gamma_M2": "1.25",
  "ui_threads_in_shear": true,
  "ui_k_cr": "0.67",
  "ui_plug_shear": true
}